
                               SUPER HUEY UH-IX 





BOOT WITHOUT BASIC, NEEDS AT LEAST 48K RAM. #1- JOYSTICK ONE PLAYER ONLY


DO NOT REMOVE GAME DISK AFTER BOOTING



CONTROLS:


KEYBOARD AND JOYSTICK:


KEYBOARD:

Uses the full keyboard compliment and three function keys.

   1-Option-onboard computer powerup.

   2-Start-Engine starter button.

   3-Select-Rotor clutch control.

  **-ESCape-Engine/off-Cut power.

        Never HIT System Reset!! 

Instruments:

 1-FRE-VHF radio aid to navigation.
 2-NAV-Compass heading from the Vor signals received.
   a-COR-may be used to apply this to the auto pilot.
   b-NAV-for manual control.
 3-RAD-activated by entering LAR command, it is line of sight from copter to
closest target.
 4-ARM-#s 1,2,3,4 are lit to indicate which rockets are armed and ready to
fire.
 5-HOM-Homeing device, range 20 miles used to return to a particular area.
 6-RES-Rescue homing signal emitted by downed personnel.
 7-Indicator Lights- Shows a disorder RETURN TO BASE.
 8-FUL-Fuel gauge
 9-OIL-Oil press. center is best.
10-TMP-Temperature, center is best.

COMPUTER KEYBOARD COMMANDS:

ABT-Abort flight.

ACS-Auto control setting.

ASN-Select new mission; 

     A- INStruction

     B- EXPloration

     C- COMbat

     D- RSC rescue

CLM-weather readings

DST-Line of Sight calculation.

GTK-Ground tracking grid.

LAR-Load, arm rockets.

MAC-Activate machine guns.

POW-Turn on power.

SAF-Send coordinates when landing or in an emergency.

RAD-Turn on radar /no weapons.

TRK- Radar tracking and targeting.

VOR-Vhf Omnidirectional Range and navigation.

VSI-Display digital vertical speed reading.





THE JOYSTICK:


Description:

The UH-1X Control operates in two modes: The cyclic mode where the stick acts
just like a flight control stick, and the collective mode, where the stick
affects blade pitch angle and throttle.

The CYCLIC mode is in effect when the fire button is  NOT  depressed.



                              CYCLIC MODE DIAGRAM
                    ______________________________________

                               + FORWARD/THRUST
                       LEFT 1         2         3 RIGHT


                            4         *          5


                       LEFT 6         7         8 RIGHT

                               - FORWARD/THRUST

===================================

                            COLLECTIVE MODE DIAGRAM
                    ______________________________________

                                 -LIFT/THRUST
                                       1


                     -THROT.2          *         3 -THROT.


                                       4
                                 + LIFT/THRUST

===================================


